US Bureau of Reclamation - Klamath Project
	Weekly Water Report - Un-corrected Data, Herald and News
If you have any questions about this report, contact Jennifer Birri at 880-2540.
UPPER KLAMATH LAKE - The surface elevation of Upper Klamath Lake as of 9/17/2007 was  4138.39 
above sea level, and its storage was 134506 a.f.  The lake elevation was down 0.12 feet from a week earlier,
  and the storage was down 7739 a.f. from a week earlier.  The lake elevation was down 0.91 feet from a 
month earlier,  and the storage was down 59582 a.f. from a month earlier.  The lake elevation was down 
0.43 feet from a year earlier,  and the storage was down 27860 a.f. from a year earlier. 
CLEAR LAKE - The surface elevation of Clear Lake as of 9/17/2007 was 4524.01 above sea level, and its 
storage was 89900 a.f.  The lake elevation was down from 4.63 feet a year earlier, and the storage was 
down 88160 a.f. from a year earlier.
GERBER RESERVOIR - The surface elevation of Gerber Reservoir as of 9/17/2007 was  4820.8 above sea 
level, and its storage was 44680 a.f.  The lake elevation was down from 4.70 feet a year earlier, and the 
storage was down 14540 a.f. from a year earlier.
	Klamath River Report
	DATE	Link  River	A Canal 	Keno 	Iron Gate 	Last Year	Link River	A Canal 	Keno	Iron Gate 
	9/10/2007	723	640	718	1,030	9/10/2006	871	637	677	1300
	9/11/2007	767	640	699	1,030	9/11/2006	811	632	724	1150
	9/12/2007	721	640	699	1,030	9/12/2006	989	657	757	1020
	9/13/2007	583	620	703	1,030	9/13/2006	769	642	761	1010
	9/14/2007	520	620	697	1,030	9/14/2006	939	625	762	1010
	9/15/2007	529	610	695	1,030	9/15/2006	826	596	766	1010
	9/16/2007	639	610	698	1,030	9/16/2006	826	580	769	997
	9/17/2007	689	660	575	1,030	9/17/2006	826	505	770	997
	Upper Klamath Lake Inflow in CFS
	9/10/2007	-921	9/10/2006	510
	9/11/2007	429	9/11/2006	781
	9/12/2007	384	9/12/2006	986
	9/13/2007	-98	9/13/2006	1,080
	9/14/2007	491	9/14/2006	575
	9/15/2007	1,464	9/15/2006	-1,214
	9/16/2007	599	9/16/2006	1,077
	9/17/2007	700	9/17/2006	674